**S-124 Edition 2.0 Change Request Log**

**Last Updated 12 September 2025**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **S-124 Part** | **Schema** | **Submitted by** | **Subject** | **Decision** | **S-124 2.X** | **Notes** | **Date** |
| S-124 FC | Warning information: information | OSI Maritime Systems | The information complex attribute should allow for multiplicity within the FC as shown in the PS. |  |  | Clarification | 2025.09.12 |
| S-124 PS | Text Placement | OSI Maritime Systems | Currently text placement is limited to English only. Proposal to add a new complex attribute |  |  |  | 2025.09.12 |
| S-124 PS | NavwarnTypeGeneral | China | Proposal to Expand NavwarnTypeGeneral to better match S-53 |  |  |  | 2025.09.12 |
| S-124 PS | Data Model Expansion | China | Proposal to add a new complex attribute to facilitate dynamic towing vessels. |  |  |  | 2025.09.12 |